FOUNDATION COURSE 4”

The Contractor shall have the option of using either Aggregate Foundation Course-D, Crushed Concrete Foundation Course or Bituminous Foundation Course; and the Contractor shall bid the pay item “Foundation Course” accordingly.

These different foundation courses may be used interchangeably throughout the project, with the exception being that the same type of foundation course shall be used across the entire width of a pavement section to provide uniform drainage across that template. The Contractor shall make every attempt to use the same type of foundation in long paving runs and any changes in foundation course type shall be approved by the Engineer.

Regardless of the type of material used it shall be obtained from Contractor sources.

Regardless of the type of material used it shall be measured and paid for as Foundation Course 4”.

Method Of Measurement

Foundation Course shall be measured as prescribed in Paragraph 3 of subsection 307.04.

Basis of Payment

Amend Subsection 307.05 of the Standard Specifications to include the following:

1. Pay Item Pay Unit

Foundation Course Square Yard