**Structure Maintenance Checklist**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Structure No.: |  |  | District: |  |  |
| Inspected By: |  |  | Date of Inspection: |  |  |
| Structure Location: |  |  | County: |  |  |
|  | |  |  | | |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Item**  **No.** | **Item** | **Maint.**  **Needed** |  | **Item**  **No.** | **Item** | **Maint.**  **Needed** |
| 1. | Repair damaged guardrail. |  |  | 9. | Fill in erosion on sideslopes and banks. |  |
| 2. | Repair/replace signs. |  |  | 10. | Fill in erosion at culvert ends. |  |
| 3. | Clean debris from expansion device. |  |  | 11. | Remove silt from barrels. |  |
| 4. | Sweep the deck/open plugged floor drains. |  |  | 12. | Remove excess silt between culvert wings. |  |
| 5. | Remove debris from girder, caps, and bearings. |  |  | 13. | Patch bridge deck. |  |
| 6. | Remove debris from channel. |  |  | 14. | Seal cracks. |  |
| 7. | Cut and remove trees from channel. |  |  | 15. | Pressure wash deck, rails, joints, and drains. |  |
| 8. | Fill in washout under approach slab. |  |  | 16. | Other: |  |

|  |
| --- |
| Remarks: |

**NDOT Form 27, July 17**