Bridge Hydraulic Cross Section Field Inspection Form
Structure No.		By		Date	
Direction of Increasing Reference Post (NE Item 217): N, NE, E, SE, S, SW, W, NW Downstream Side of Bridge: Left, Right
Note: Measurements are to be taken on the downstream side of the bridge at each support and change in topography. At least one cross section is required for every non-culvert structure over water. See the cross section input guidance on the Bridge Division web page for more information. This form is not required for submittal and is provided for data collection support only.

Use this table if structural elevations are taken in the field. Add notes as needed for additional supports.Location
Distance (ft)
Elev (ft)
Abut 1


Pier 1


Pier 2


Pier 3


Pier 4


Abut 2



Location
Distance (ft)
Elev(ft)





















Location of base measurement 		Elevation Basis: Assumed, Survey, Plans
If base measurement is at top of rail, add rail height in ft. 	
This area is for recorded drop measurements at each support or change of topography.Location
Distance (ft)
Drop (ft)
Abut 1







































Location
Distance (ft)
Drop (ft)









































BR Form 384 July 2026
